34d3539eab8ce545251995b939bba674
ignore
This software comes with  ABSOLUTELY NO WARRANTY.  This
is free software and you are welcome to redistribute it
under the conditions of the GNU GENERAL PUBLIC LICENSE.
See the file "COPYING" for further information.

Opening rs02-tmp.iso
ExamineUDF(File: rs02-tmp.iso)
 Examining the ISO file system...
  Sector 16:
   Volume descriptor type    = 1
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> primary volume descriptor:
    System identifier         : |                                |
    Volume identifier         : |RANDOM IMAGE                    |
    Volume space size         : 30150 sectors
    Volume set size           : 1
    Volume sequence size      : 1
    Logical block size        : 2048
    Path table size           : 10 bytes
    L-Path table location     : 19
    Opt L-Path table location : 0
    M-Path table location     : 20
    Opt M-Path table location : 0
    Volume creation date/time : 16-07-2006 10:35:46.23
    Volume modification d/t   : 16-07-2006 10:35:46.23
    Volume expiration d/t     : 16-07-2106 10:35:46.23
    Volume effective d/t      : 16-07-2006 10:35:46.23
    File structure version    : 1
  Sector 17:
   Volume descriptor type    = 2
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> supplementary volume descriptor: *skipped*
  Sector 18:
   Volume descriptor type    = 255
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> volume descriptor set terminator;
      end of ISO file system parsing.
 Examining the UDF file system...
  not yet implemented.

ExamineECC() started
...trying RS01
...trying RS02
RS02Recognize: file rs02-tmp.iso
try_sector: trying sector 30150
try_sector: no cookie, skipping current modulo
try_sector: trying sector 30000
try_sector: header at 30000: magic cookie found
try_sector: CRC okay
GetImageFingerprint(16): read & cached
try_sector: fingerprint okay, header good
Root sector search at -150 successful
...augmented image found
Expected size calculated from ecc header: 34932
--> confirmed layout variant 1
Calculated layout for RS02 image:
data sectors      = 30000
crc sectors       = 59
protected sectors = 30061 (incl. 2 hdr sectors)
reed solomon secs = 4795 (35 roots, 220 data)
header repeats    = 38 (using modulo 128)
added sectors     = 4932
total image size  = 34932
medium capacity   = n.a.

Interleaving layout:
137 sectors per ecc layer
first layer sector with CRC data 136 (sector# 30002)

GetImageFingerprint(16): cached
: 34932 medium sectors.
RS02LayoutFromImage(): returning cached layout

Fix mode(RS02): Repairable sectors will be fixed in the image.
Good! All sectors are already present.

Summary of processed sectors:
0 damaged sectors
0 CRC errors
0 of 280576 ecc blocks damaged (0 / 137 sectors)
all data sectors processed
all  crc sectors processed
all  ecc sectors processed
