9c8681ccde613b9edae6fd148d76f11b
ignore
This software comes with  ABSOLUTELY NO WARRANTY.  This
is free software and you are welcome to redistribute it
under the conditions of the GNU GENERAL PUBLIC LICENSE.
See the file "COPYING" for further information.
# *** OpenImageFromDevice(sim-cd) ***
# InquireDevice returned: Simulated CD drive 1.00

Device: sim-cd, Simulated CD drive 1.00
# *** query_type(Simulated CD drive 1.00, 0) ***
# *** get_configuration(Simulated CD drive 1.00) ***
# 8 data len, 9 current
-> profile 9: CD-R
# trying READ DISC INFORMATION for size
# size returned is 32
# trying READ DISC INFORMATION for real info
0000: 00 20 1e 00 00 00 00 00  00 00 00 00 00 00 00 00  . ...... ........ 
0010: 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00  ........ ........ 
# status is 1e, disc type 0
#CD: starting media probe
#CD: querying size of READ TOC/PMA/ATIP (for TOC)
#CD: size returned is 12
#CD: querying real READ TOC/PMA/ATIP (for TOC)
0000: 00 0a 00 00 00 14 00 00  00 00 00 00              ........ ....
#CD: control is 0x14
#CD: querying size of READ TOC/PMA/ATIP (for full TOC)
# Warning: Realigning length from 26 to 24
#CD: size returned is 24
#CD: querying real READ TOC/PMA/ATIP (for full TOC)
0000: 00 18 00 01 00 00 00 a0  00 00 00 00 00 00 00 00  ........ ........ 
0010: 00 00 00 00 00 00 00 00                           ........ 
#CD: 1 sessions
#CD: CD medium detected, type: CD-R mode 1
# query_type() returned.
# deciding reading strategy...
Using READ CD.
GetImageFingerprint(16): not readable

ExamineUDF(Device: Simulated CD drive 1.00)
 Examining the ISO file system...
  Sector 16: unreadable
  Sector 17:
   Volume descriptor type    = 2
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> supplementary volume descriptor: *skipped*
  Sector 18:
   Volume descriptor type    = 255
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> volume descriptor set terminator;
      end of ISO file system parsing.
 Examining the UDF file system...
  not yet implemented.

# *** read_capacity(Simulated CD drive 1.00) ***
 -> 24989
ExamineECC() started
...trying RS01
...trying RS02
RS02Recognize: medium sim-cd
RS02Recognize: skipping exhaustive RS02 search
...trying RS03
RS03RecognizeImage: medium sim-cd
FindRS03HeaderInImage: medium sim-cd
 . NO ISO structures found!
RS03RecognizeImage: No EH, entering exhaustive search
Warning: image size set to 25000 for debugging!
.. trying layer size 98
Scanning layers for signatures.
- layer slice 0
** Success: sector 21070, rediscovered format with 39 roots
...augmented image found
# Calling query_size()
# *** query_size(Simulated CD drive 1.00) ***
Medium size obtained from ECC header: 24990 sectors
# returned: 24990 sectors
Medium: CD-R mode 1, 24990 sectors, Ecc.

Creating new rs03i-tmp.iso image.
Reading CRC information from ecc data (RS03) ... Calculated layout for RS03 image:
data sectors      = 21000
data padding      = 68
layer size        = 98
total sectors     = 24990
medium capacity   = 0
header position   = 21000
first CRC sector  = 21070
first ECC sector  = 21168
ndata             = 216
nroots            = 39 (18.1%)

done.
Sector 16, try 1: Medium Error; Unrecovered read error.
Sector 16: Medium Error; Unrecovered read error. Skipping 15 sectors.

16 unreadable sectors.
CrcBuf contents, image path none (medium):
  crcSize: 24990, dataSectors: 21000, coveredSectors: 21070, allSectors: 24990
  md5State: invalid
  fp sector: 16; invalid
  missing crcs: 0
