ignore
ignore
This software comes with  ABSOLUTELY NO WARRANTY.  This
is free software and you are welcome to redistribute it
under the conditions of the GNU GENERAL PUBLIC LICENSE.
See the file "COPYING" for further information.

ExamineUDF(File: rs02-master.iso)
 Examining the ISO file system...
  Sector 16:
   Volume descriptor type    = 1
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> primary volume descriptor:
    System identifier         : |                                |
    Volume identifier         : |RANDOM IMAGE                    |
    Volume space size         : 30000 sectors
    Volume set size           : 1
    Volume sequence size      : 1
    Logical block size        : 2048
    Path table size           : 10 bytes
    L-Path table location     : 19
    Opt L-Path table location : 0
    M-Path table location     : 20
    Opt M-Path table location : 0
    Volume creation date/time : 16-07-2006 10:35:46.23
    Volume modification d/t   : 16-07-2006 10:35:46.23
    Volume expiration d/t     : 16-07-2106 10:35:46.23
    Volume effective d/t      : 16-07-2006 10:35:46.23
    File structure version    : 1
  Sector 17:
   Volume descriptor type    = 2
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> supplementary volume descriptor: *skipped*
  Sector 18:
   Volume descriptor type    = 255
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> volume descriptor set terminator;
      end of ISO file system parsing.
 Examining the UDF file system...
  not yet implemented.

ExamineECC() started
...trying RS01
...trying RS02
RS02Recognize: file rs02-master.iso
try_sector: trying sector 30000
try_sector: header at 30000: magic cookie found
try_sector: CRC okay
GetImageFingerprint(16): read & cached
try_sector: fingerprint okay, header good
Root sector search at +0 successful
...augmented image found
Expected size calculated from ecc header: 34932
--> confirmed layout variant 1
Calculated layout for RS02 image:
data sectors      = 30000
crc sectors       = 59
protected sectors = 30061 (incl. 2 hdr sectors)
reed solomon secs = 4795 (35 roots, 220 data)
header repeats    = 38 (using modulo 128)
added sectors     = 4932
total image size  = 34932
medium capacity   = n.a.

Interleaving layout:
137 sectors per ecc layer
first layer sector with CRC data 136 (sector# 30002)

GetImageFingerprint(16): cached
RS03RecognizeFile(): examining rs02-tmp.ecc
RS03RecognizeFile(): ecc header found
GetImageFingerprint(16): cached

rs02-master.iso present.
rs02-tmp.ecc present.
CalcRS03Layout(): removed cached layout from other codec
Calculated layout for RS03 file:
data sectors      = 34932
data padding      = 0
layer size        = 150
total sectors     = 38084
medium capacity   = 0
header position   = 0
first CRC sector  = 2
first ECC sector  = 152
ndata             = 235
nroots            = 20 ( 8.5%)


Error correction properties:
- type             : Error correction file
- method           : RS03, 20 roots,  8.5% redundancy.
- created by       : dvdisaster-0.80
- requires         : dvdisaster-0.79
- data md5sum      : none available
* fingerprint match: MISMATCH - .iso and .ecc don't belong together!

Data integrity:
- sectors          : 34932 in image; 3152 in ecc file
CalcRS03Layout(): returning cached layout (file)
* CRC error, sector: 16
* suspicious image : all sectors present, but 1 CRC errors
  ... data section   : 0 sectors missing; 1 CRC errors
  ... crc section    : 0 sectors missing
  ... ecc section    : 0 sectors missing
* Ecc block test   : 149 good, 1 bad; 1 bad sub blocks
- erasure counts   :  avg =  1.0; worst = 1 per ecc block.
- prognosis        : 38084 of 38084 sectors recoverable (100.0%)
FreeCrcBuf - buffer cleared
