ignore
ignore
This software comes with  ABSOLUTELY NO WARRANTY.  This
is free software and you are welcome to redistribute it
under the conditions of the GNU GENERAL PUBLIC LICENSE.
See the file "COPYING" for further information.
# *** OpenImageFromDevice(sim-cd) ***
# InquireDevice returned: Simulated CD drive 1.00

Device: sim-cd, Simulated CD drive 1.00
# *** query_type(Simulated CD drive 1.00, 0) ***
# *** get_configuration(Simulated CD drive 1.00) ***
# 8 data len, 9 current
-> profile 9: CD-R
# trying READ DISC INFORMATION for size
# size returned is 32
# trying READ DISC INFORMATION for real info
0000: 00 20 1e 00 00 00 00 00  00 00 00 00 00 00 00 00  . ...... ........ 
0010: 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00  ........ ........ 
# status is 1e, disc type 0
#CD: starting media probe
#CD: querying size of READ TOC/PMA/ATIP (for TOC)
#CD: size returned is 12
#CD: querying real READ TOC/PMA/ATIP (for TOC)
0000: 00 0a 00 00 00 14 00 00  00 00 00 00              ........ ....
#CD: control is 0x14
#CD: querying size of READ TOC/PMA/ATIP (for full TOC)
# Warning: Realigning length from 26 to 24
#CD: size returned is 24
#CD: querying real READ TOC/PMA/ATIP (for full TOC)
0000: 00 18 00 01 00 00 00 a0  00 00 00 00 00 00 00 00  ........ ........ 
0010: 00 00 00 00 00 00 00 00                           ........ 
#CD: 1 sessions
#CD: CD medium detected, type: CD-R mode 1
# query_type() returned.
# deciding reading strategy...
Using READ CD.
GetImageFingerprint(16): read & cached

ExamineUDF(Device: Simulated CD drive 1.00)
 Examining the ISO file system...
  Sector 16:
   Volume descriptor type    = 1
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> primary volume descriptor:
    System identifier         : |                                |
    Volume identifier         : |RANDOM IMAGE                    |
    Volume space size         : 274300 sectors
    Volume set size           : 1
    Volume sequence size      : 1
    Logical block size        : 2048
    Path table size           : 10 bytes
    L-Path table location     : 19
    Opt L-Path table location : 0
    M-Path table location     : 20
    Opt M-Path table location : 0
    Volume creation date/time : 16-07-2006 10:35:46.23
    Volume modification d/t   : 16-07-2006 10:35:46.23
    Volume expiration d/t     : 16-07-2106 10:35:46.23
    Volume effective d/t      : 16-07-2006 10:35:46.23
    File structure version    : 1
  Sector 17:
   Volume descriptor type    = 2
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> supplementary volume descriptor: *skipped*
  Sector 18:
   Volume descriptor type    = 255
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> volume descriptor set terminator;
      end of ISO file system parsing.
 Examining the UDF file system...
  not yet implemented.

# *** read_capacity(Simulated CD drive 1.00) ***
 -> 357654
ExamineECC() started
...trying RS01
...trying RS02
RS02Recognize: medium sim-cd
try_sector: trying sector 274300
try_sector: header at 274300: magic cookie found
try_sector: CRC okay
GetImageFingerprint(16): cached
try_sector: fingerprint okay, header good
Root sector search at +0 successful
...augmented image found
Pre-0.79.5 RS02 header.
Expected size taken from image->dh: 357655/1
NOTE: header modulo glitch fixed
Calculated layout for RS02 image:
data sectors      = 274300
crc sectors       = 536
protected sectors = 274838 (incl. 2 hdr sectors)
reed solomon secs = 82777 (59 roots, 196 data)
header repeats    = 20 (using modulo 4096)
added sectors     = 83355
total image size  = 357655
medium capacity   = n.a.

Interleaving layout:
1403 sectors per ecc layer
first layer sector with CRC data 717 (sector# 274302)

# Calling query_size()
# *** query_size(Simulated CD drive 1.00) ***
Medium size obtained from ECC header: 357655 sectors
# returned: 357655 sectors
Medium "Random Image": CD-R mode 1, 357655 sectors, Ecc, created 16-07-2006.

Scanning medium for read errors.
Reading CRC information from ecc data (RS02) ... RS02LayoutFromImage(): returning cached layout
done.
GOOD Data md5sum
GOOD CRC md5sum
GOOD ECC md5sum

All sectors successfully read. Checksums match.
CrcBuf contents, image path none (medium):
  crcSize: 357655, dataSectors: 274300, coveredSectors: 274300, allSectors: 357655
  md5State: data_complete image_complete
  data: aae7e725ff308877a45210bfd0b737f7
  full: 61fc6058150dd48c46648c2fe85f8bd7
  fp sector: 16; 48a5a2186ffe363bee215f406d033aa7
  missing crcs: 0
