ignore
ignore
This software comes with  ABSOLUTELY NO WARRANTY.  This
is free software and you are welcome to redistribute it
under the conditions of the GNU GENERAL PUBLIC LICENSE.
See the file "COPYING" for further information.
# *** OpenImageFromDevice(sim-cd) ***
# InquireDevice returned: Simulated CD drive 1.00

Device: sim-cd, Simulated CD drive 1.00
# *** query_type(Simulated CD drive 1.00, 0) ***
# *** get_configuration(Simulated CD drive 1.00) ***
# 8 data len, 9 current
-> profile 9: CD-R
# trying READ DISC INFORMATION for size
# size returned is 32
# trying READ DISC INFORMATION for real info
0000: 00 20 1e 00 00 00 00 00  00 00 00 00 00 00 00 00  . ...... ........ 
0010: 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00  ........ ........ 
# status is 1e, disc type 0
#CD: starting media probe
#CD: querying size of READ TOC/PMA/ATIP (for TOC)
#CD: size returned is 12
#CD: querying real READ TOC/PMA/ATIP (for TOC)
0000: 00 0a 00 00 00 14 00 00  00 00 00 00              ........ ....
#CD: control is 0x14
#CD: querying size of READ TOC/PMA/ATIP (for full TOC)
# Warning: Realigning length from 26 to 24
#CD: size returned is 24
#CD: querying real READ TOC/PMA/ATIP (for full TOC)
0000: 00 18 00 01 00 00 00 a0  00 00 00 00 00 00 00 00  ........ ........ 
0010: 00 00 00 00 00 00 00 00                           ........ 
#CD: 1 sessions
#CD: CD medium detected, type: CD-R mode 1
# query_type() returned.
# deciding reading strategy...
Using READ CD.
GetImageFingerprint(16): read & cached

ExamineUDF(Device: Simulated CD drive 1.00)
 Examining the ISO file system...
  Sector 16:
   Volume descriptor type    = 1
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> primary volume descriptor:
    System identifier         : |                                |
    Volume identifier         : |RANDOM IMAGE                    |
    Volume space size         : 30000 sectors
    Volume set size           : 1
    Volume sequence size      : 1
    Logical block size        : 2048
    Path table size           : 10 bytes
    L-Path table location     : 19
    Opt L-Path table location : 0
    M-Path table location     : 20
    Opt M-Path table location : 0
    Volume creation date/time : 16-07-2006 10:35:46.23
    Volume modification d/t   : 16-07-2006 10:35:46.23
    Volume expiration d/t     : 16-07-2106 10:35:46.23
    Volume effective d/t      : 16-07-2006 10:35:46.23
    File structure version    : 1
  Sector 17:
   Volume descriptor type    = 2
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> supplementary volume descriptor: *skipped*
  Sector 18:
   Volume descriptor type    = 255
   Volume descriptor version = 1
   Standard identifier       = CD001
   -> volume descriptor set terminator;
      end of ISO file system parsing.
 Examining the UDF file system...
  not yet implemented.

# *** read_capacity(Simulated CD drive 1.00) ***
 -> 34977
ExamineECC() started
...trying RS01
...trying RS02
RS02Recognize: medium sim-cd
try_sector: trying sector 30000
try_sector: header at 30000: magic cookie found
try_sector: CRC okay
GetImageFingerprint(16): cached
try_sector: fingerprint okay, header good
Root sector search at +0 successful
...augmented image found
Expected size calculated from ecc header: 34932
--> confirmed layout variant 1
Calculated layout for RS02 image:
data sectors      = 30000
crc sectors       = 59
protected sectors = 30061 (incl. 2 hdr sectors)
reed solomon secs = 4795 (35 roots, 220 data)
header repeats    = 38 (using modulo 128)
added sectors     = 4932
total image size  = 34932
medium capacity   = n.a.

Interleaving layout:
137 sectors per ecc layer
first layer sector with CRC data 136 (sector# 30002)

# Calling query_size()
# *** query_size(Simulated CD drive 1.00) ***
Medium size obtained from ECC header: 34932 sectors
# returned: 34932 sectors
Medium "Random Image": CD-R mode 1, 34932 sectors, Ecc, created 16-07-2006.

Scanning medium for read errors.
Reading CRC information from ecc data (RS02) ... RS02LayoutFromImage(): returning cached layout
done.
GOOD Data md5sum
GOOD CRC md5sum
GOOD ECC md5sum

All sectors successfully read. Checksums match.
CrcBuf contents, image path none (medium):
  crcSize: 34932, dataSectors: 30000, coveredSectors: 30000, allSectors: 34932
  md5State: data_complete image_complete
  data: cbadac3ca7b6e9bccfc889b7eaded254
  full: 814f4c46fbb687eb43613fdfde9458cf
  fp sector: 16; abe80d3600553a8dce779713afd94f3c
  missing crcs: 0
